Purpose: Test out different states and their movement depending on RF signals. Incorporates a battery

Status: Static test completed. WIP for dynamic, battery powered, in the field test